
[Version]
Signature="$Chicago$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%CGimagetech%
CatalogFile=CGUSB2.cat
DriverVer=10/28/2014,1.0

[SourceDisksNames]
1=%CGUSB2%,,,

[SourceDisksFiles]
CGUSB2.sys = 1

[DestinationDirs]
CGUSB2.Files.Ext = 10,System32\Drivers


[Manufacturer]
%CGimagetech%=Device,NT,NTx86,NTamd64


[Device.NT]

%VID_0828&PID_1002.DeviceDesc%=CGUSB2, USB\VID_0828&PID_1002
%VID_0920&PID_0500.DeviceDesc%=CGUSB2, USB\VID_0920&PID_0500


[Device.NTx86]

%VID_0828&PID_1002.DeviceDesc%=CGUSB2, USB\VID_0828&PID_1002
%VID_0920&PID_0500.DeviceDesc%=CGUSB2, USB\VID_0920&PID_0500


[Device.NTamd64]

%VID_0828&PID_1002.DeviceDesc%=CGUSB2, USB\VID_0828&PID_1002
%VID_0920&PID_0500.DeviceDesc%=CGUSB2, USB\VID_0920&PID_0500


[CGUSB2.NT]
CopyFiles=CGUSB2.Files.Ext
AddReg=CGUSB2.AddReg


[CGUSB2.NT.Services]
Addservice = CGUSB2,2,CGUSB2.AddService


[CGUSB2.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,CGUSB2.sys
HKR,,DriverBase,,CGUSB2.sys
HKR,"Parameters","MaximumTransferSize",0x10001,65536
HKR,"Parameters","DebugLevel",0x10001,2
HKR,,FriendlyName,,%CGUSB2_SvcDesc%

[CGUSB2.AddService]
DisplayName    = %CGUSB2_SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\CGUSB2.sys
AddReg         = CGUSB2.AddReg
LoadOrderGroup = Base

[CGUSB2.Files.Ext]
CGUSB2.sys

;-------------- WDF Coinstaller installation
[SourceDisksFiles]
WdfCoInstaller01009.dll=1 

[DestinationDirs]
CoInstaller_CopyFiles = 11

[CGUSB2.NTamd64.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CGUSB2.NTx86.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
WdfCoInstaller01009.dll

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[CGUSB2.NTamd64.Wdf]
KmdfService = CGUSB2, CGUSB2_wdfsect

[CGUSB2.NTx86.Wdf]
KmdfService = CGUSB2, CGUSB2_wdfsect

[CGUSB2_wdfsect]
KmdfLibraryVersion = 1.9


[Strings]
CGUSB2_Provider    = "CGimagetech"
CGUSB2_Company     = "CGimagetech"
CGUSB2_Description = "CGimagetech USB2.0 Driver"
CGUSB2_DisplayName = "CGimagetech USB2.0 Driver"
CGUSB2_Install     = "CGimagetech USB2.0 Driver"

VID_0920&PID_0500.DeviceDesc="TS Camera3.0"
VID_0828&PID_1002.DeviceDesc="TS Camera2.0"






